Ealead Coorpicker V2.01---电子制造PCB图像SMT\AI高精度编程坐标提取软件

2015年10月最新发布 Ealead Coorpicker V2.01
=====================================================================================
>>>软件概述
Coorpicker是专业的PCB图像SMT\AI离线编程坐标提取软件，主要功能包括从PCB图像中提取SMT及AI编程坐标数据，支持全自动和手动两种方式快速提取坐标数据，并且具备强大的图像处理能力，能从扫描仪中直接获取图像以及支持读取常用十几种图像格式文件和RS-274X格式Gerber文件。

>>>新特性 
·2015年10月 发布Coorpicker V2.01 
1.支持直接读取PADS、CADSTAR、Allegro/OrCAD等RS-274X Gerber文件。
2.支持Windows 8界面风格。
3.修正一些程序错误。
·2015年09月 发布Coorpicker V2.00 
1.支持直接读取Protel RS-274X Gerber文件。
2.修正一些程序错误。
·2015年04月 发布Coorpicker V1.58 
1.修正一些程序错误。
·2014年05月 发布Coorpicker 2014 V1.56 
1.增加测量角度功能。
2.修正一些程序错误。
·2013年11月 发布Coorpicker 2014 V1.55 
1.增加大十字光标颜色设置等选项。
2.修正一些程序错误。
·2012年09月 发布Coorpicker 2012 V1.53 
1.增加自动提取坐标功能。
2.支持导入坐标数据及重画元件位置图,方便您进行新(旧)坐标与PCB图像对比。
3.修正一些程序错误。
·2012年07月 发布Coorpicker 2012 V1.52 
修正一些程序错误。
·2011年08月 发布Coorpicker 2012 V1.50 
1.增加图像放大窗口大十字光标显示，方便快速提取坐标。
2.修正一些程序错误。
3.软件界面采用Office 2010风格。
·2010年09月 发布Coorpicker 2010 V1.40 
1.元件中心"+”号大小自动适应显示。
2.增加自动浏览元件功能。 
3.修正元件浏览显示不准确错误。
4.改进坐标提取文件输出结构，优化文件空间大小，修正不同分辨率图像文件保存后坐标不准确错误。 
5.软件界面采用Win 7风格。
·2009年12月 发布Coorpicker 2010 V1.30
1.元件中心增加“+”号显示。
2.改进图像旋转错误。
3.提高二次坐标校正精度。
4.修正Excel文件输出功能。
5.软件界面采用Office 2007风格。
·2008年05月 发布Coorpicker V1.20
改进部分程序功能，增加图像比例自动计算功能。
·2007年05月 发布Coorpicker V1.10
改进软件界面及修正部分程序错误。
·2006年02月 发布Coorpicker V1.00
本次所发布的属本软件的第一个版本。

>>>系统配置要求 
1.操作系统:Windows 2000\XP以上。
2.剩余硬盘空间:50MB以上。
3.内存配置:256MB以上。
4.显示器分辨率:1024*768以上。 

>>>软件许可协议
在您使用本软件前，请您认真阅读并理解下列条款：
1.未经许可，您不得修改、出租、销售、散布、转让本软件的任何部分，并同意防止非法拷贝本软件。
2.您不得对本软件进行反向工程、反向编译或反汇编操作。
3.您不得授权或允许对超过一个用户使用本软件。
4.未经许可，您不得将本软件作为商业用途。
5.任何情况下，作者将不承担由于任何未知因素导致您无法使用本软件所造成的任何损失。
6.如果您已安装使用本软件，则表示您已经同意遵守本软件协议，否则请您立即删除本软件。

----------------------------------------------------------------------------------------
版权所有(C)2015 赢立软件科技(Ealead) 保留所有权利 
技术支持 赢立电子辅助软件开发团队 电话:+8613695245328 QQ:190130616  
网址:http://ealead.ucoz.com 客服邮箱:ealeadservice@163.com

----------------------------------------------------------------------------------------

Ealead Coorpicker V2.01---PCB Image Coordinate Data Extraction Tool for SMT and AI
========================================================================================
>>>Introduction
Coorpicker is a professional software of coordinate data extraction for SMT or AI offline programming. With Coorpicker, you can quickly and easily pick the high-accuracy coordinate data from PCB image. Coorpicker also has the powerful image processing abilities and it supports to read more than 10 various format image files and RS-274X gerber file.

>>>What's new
·Coorpicker V2.01, released on October 2015. 
1. Supports to read PADS、CADSTAR、Allegro/OrCAD RS-274X gerber file.
2. Adopt Windows 8 style in the program interface.
3. Correct some program bugs.
·Coorpicker V2.00, released on September 2015. 
1. Supports to read Protel RS-274X gerber file.
2. Correct some program bugs.
·Coorpicker V1.58, released on April 2015. 
1. Correct some program bugs. 
·Coorpicker 2014 V1.56, released on May 2014. 
1. Add the function of angle measurement.
2. Correct some program bugs. 
·Coorpicker 2014 V1.55, released on November 2013. 
1. Add the options setup for big cross and pad mark color.
2. Correct some program bugs. 
·Coorpicker 2012 V1.53, released on September 2012. 
1. Add the function of pick the component coordinate data by automatic.
2 Supports to import coordinate data from file and redraw all components location diagram, helps you quickly compare the difference between the new (old) coordinate data and old (new) PCB image.
3. Correct some program bugs. 
·Coorpicker 2012 V1.52, released on July 2012. 
Correct some program bugs. 
·Coorpicker 2012 V1.50, released on August 2011. 
1. Add the big size of cross cursor in zoom in view window. 
2. Correct some program bugs. 
3. Adopt Office 2010 style in the program interface. 
·Coorpicker 2010 V1.40, released on September 2010. 
1. The size of "+" in the center of component can be auto adjusted. 
2. Add the function of browse components by automatic. 
3. Improve the file structure of PIC file. 
4. Adopt Win 7 style in the program interface. 
5. Correct some program bugs.
·Coorpicker 2010 V1.30, released on December 2009. 
1. Add the "+" in the center of component. 
2. Correct the bug of image rotation. 
3. Improve the accuracy of coordinate adjustment. 
4. Improve the Excel file output function. 
5. Adopt Office 2007 style in the program interface. 
·Coorpicker V1.20, released on May 2008. 
Add the function of calculate the image rate by automatic. 
·Coorpicker V1.10, released on May 2007.
Improve the program interface and correct some program bugs. 
·Coorpicker V1.00, released on February 2006. 
The first version of Coorpicker, supports to pick the coordinate data from PCB image.

>>>System requirements 
1. Windows 2000 or XP OS or later. 
2. 50MB or more available disk space. 
3. 256MB or more system memory. 
4. 1024*768 or higher resolution monitor.

>>>Software License Agreement
? Before to use this software, you should to read below license agreement carefully and understand these conditions:
1. You may not modify, rent, sell, distribute or transfer any part of the software without authorized, and you agree to prevent unauthorized copying of the software.
2. You may not reverse engineer, decompile or disassemble the software. 
3. You may not sublicense or permit simultaneous use of the software by more than one user.
4. You may not use this software for business without authorized.
5. In any case, the author won't undertake any responsibility of the results effected by that you cannot use this software cause by any unknown reasons.
6. If you installed and use this computer program, that meant you had already agreed to accept this software license agreement, otherwise you should to uninstall and delete this software immediately.
 
----------------------------------------------------------------------------------------
Copyright(C)2015 Ealead Corporation. All rights reserved. 
Technology Support: Ealead Software Development Team  Phone: +8613695245328 QQ: 190130616  
Web Site:http: //ealead.ucoz.com E-Mail:ealeadservice@163.com
